Next: Standard Replies, Up: Remote Protocol

### D.1 Overview

There may be occasions when you need to know something about the protocol—for example, if there is only one serial port to your target machine, you might want your program to do something special if it recognizes a packet meant for gdb.

In the examples below, ‘`->`’ and ‘`<-`’ are used to indicate transmitted and received data, respectively.

All gdb commands and responses (other than acknowledgments and notifications, see Notification Packets) are sent as a packet. A packet is introduced with the character ‘`$`’, the actual packet-data, and the terminating character ‘`#`’ followed by a two-digit checksum:

         $packet-data#checksum

The two-digit checksum is computed as the modulo 256 sum of all characters between the leading ‘`$`’ and the trailing ‘`#`’ (an eight bit unsigned checksum).

Implementors should note that prior to gdb 5.0 the protocol specification also included an optional two-digit sequence-id:

         $sequence-id:packet-data#checksum

That sequence-id was appended to the acknowledgment. gdb has never output sequence-ids. Stubs that handle packets added since gdb 5.0 must not accept sequence-id.

When either the host or the target machine receives a packet, the first response expected is an acknowledgment: either ‘`+`’ (to indicate the package was received correctly) or ‘`-`’ (to request retransmission):

         -> $packet-data#checksum
         <- +

The ‘`+`’/‘`-`’ acknowledgments can be disabled once a connection is established. See Packet Acknowledgment, for details.

The host (gdb) sends commands, and the target (the debugging stub incorporated in your program) sends a response. In the case of step and continue commands, the response is only sent when the operation has completed, and the target has again stopped all threads in all attached processes. This is the default all-stop mode behavior, but the remote protocol also supports gdb's non-stop execution mode; see Remote Non-Stop, for details.

packet-data consists of a sequence of characters with the exception of ‘`#`’ and ‘`$`’ (see ‘`X`’ packet for additional exceptions).

Fields within the packet should be separated using ‘`,`’ ‘`;`’ or ‘`:`’. Except where otherwise noted all numbers are represented in hex with leading zeros suppressed.

Implementors should note that prior to gdb 5.0, the character ‘`:`’ could not appear as the third character in a packet (as it would potentially conflict with the sequence-id).

Binary data in most packets is encoded either as two hexadecimal digits per byte of binary data. This allowed the traditional remote protocol to work over connections which were only seven-bit clean. Some packets designed more recently assume an eight-bit clean connection, and use a more efficient encoding to send and receive binary data.

The binary data representation uses `7d` (ascii ‘`}`’) as an escape character. Any escaped byte is transmitted as the escape character followed by the original character XORed with `0x20`. For example, the byte `0x7d` would be transmitted as the two bytes `0x7d 0x5d`. The bytes `0x23` (ascii ‘`#`’), `0x24` (ascii ‘`$`’), and `0x7d` (ascii ‘`}`’) must always be escaped. Responses sent by the stub must also escape `0x2a` (ascii ‘`*`’), so that it is not interpreted as the start of a run-length encoded sequence (described next).

Response data can be run-length encoded to save space. Run-length encoding replaces runs of identical characters with one instance of the repeated character, followed by a ‘`*`’ and a repeat count. The repeat count is itself sent encoded, to avoid binary characters in data: a value of n is sent as n`+29`. For a repeat count greater or equal to 3, this produces a printable ascii character, e.g. a space (ascii code 32) for a repeat count of 3. (This is because run-length encoding starts to win for counts 3 or more.) Thus, for example, ‘`0*` ’ is a run-length encoding of “0000”: the space character after ‘`*`’ means repeat the leading `0` `32 - 29 = 3` more times.

The printable characters ‘`#`’ and ‘`$`’ or with a numeric value greater than 126 must not be used. Runs of six repeats (‘`#`’) or seven repeats (‘`$`’) can be expanded using a repeat count of only five (‘`"`’). For example, ‘`00000000`’ can be encoded as ‘`0*"00`’.

In describing packets (and responses), each description has a template showing the overall syntax, followed by an explanation of the packet's meaning. We include spaces in some of the templates for clarity; these are not part of the packet's syntax. No gdb packet uses spaces to separate its components. For example, a template like ‘`foo bar baz`’ describes a packet beginning with the three ASCII bytes ‘`foo`’, followed by a bar, followed directly by a baz. gdb does not transmit a space character between the ‘`foo`’ and the bar, or between the bar and the baz.

We place optional portions of a packet in [square brackets]; for example, a template like ‘`c [addr]`’ describes a packet beginning with the single ASCII character ‘`c`’, possibly followed by an addr.