6.9. Supported Board Files
Prev | Chapter 6. Sourcery CodeBench Debug Sprite | Next

## 6.9. Supported Board Files

The Sourcery CodeBench Debug Sprite for ARM EABI includes support for the following target boards. Specify the appropriate `board-file` as an argument when invoking the Sprite from the command line.

Board | Config
--- | ---
Altera Cyclone III Cortex-M1 | `cycloneiii-cm1`
ARMulator (RDI) | `armulator`
Xilinx Zynq-7000 | `zynq7000`

Prev | Up | Next
6.8. Debugging a Remote Board | Home | 6.10. Board File Syntax