Next: Architectures, Previous: Embedded OS, Up: Configurations

### 21.3 Embedded Processors

This section goes into details specific to particular embedded configurations.

Whenever a specific embedded processor has a simulator, gdb allows to send an arbitrary command to the simulator.

`sim` command
  Send an arbitrary command string to the simulator. Consult the documentation for the specific simulator in use for information about acceptable commands.