Previous: Blackfin Syntax, Up: Blackfin-Dependent

#### 9.5.3 Directives

The following directives are provided for compatibility with the VDSP assembler.

`.byte2`
  Initializes a two byte data object.

  This maps to the `.short` directive.

`.byte4`
  Initializes a four byte data object.

  This maps to the `.int` directive.

`.db`
  Initializes a single byte data object.

  This directive is a synonym for `.byte`.

`.dw`
  Initializes a two byte data object.

  This directive is a synonym for `.byte2`.

`.dd`
  Initializes a four byte data object.

  This directive is a synonym for `.byte4`.

`.var`
  Define and initialize a 32 bit data object.