6.5. Remote Debug Interface Devices
Prev | Chapter 6. Sourcery CodeBench Debug Sprite | Next

## 6.5. Remote Debug Interface Devices

Remote Debug Interface (RDI) devices are supported. The RDI device URL accepts no hostname, port or path components, so the `device-url` is specified as follows:

    rdi:[///][?device-options]

The following `device-options` are required:

`rdi-library=`library``

  Specify the library (DLL or shared object) implementing the RDI target you wish to use.

`rdi-config=`configfile``

  Specify a file containing configuration information for `library`. The format of this file is specific to the RDI library you are using, but tends to constitute a list of ``key`=`value`` pairs. Consult the documentation of your RDI library for details.

Prev | Up | Next
6.4. Sourcery CodeBench Debug Sprite Options | Home | 6.6. Actel FlashPro Devices